{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["000000","내역서"],"not_rendered":{"external_links":25,"defined_names":86},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"000000","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"내역서","index":1,"n_rows":22,"n_cols":12,"rows_kept":22,"merged":[[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,0,6],[0,7,0,8],[0,9,0,10],[0,11,1,11]],"flags":["formulas_cached_only"]}
[null,"품          명","규        격","단위","수량","재      료      비",null,"노     무     비",null,"     계   ",null,"비 고"]
[{"$nulls":5},"단 가","금      액","단 가","금      액","단 가","금    액"]
[null,"- 무대기계장치  집계표- "]
[null,"MAIN CURTAIN","19,000Lx11,000H                         / 7.5kW x 4P","SET",1,null,0,null,0,null,0]
[null,"NO.\t1, 2, 3, 5, 6, 9, 11, 12, 13, 14, 15, 16, 18 SET BATTEN_신설","18,000L_EXT 1,000 / 7.5kW x 4P","SET",13,null,0,null,0,null,0]
[null,"NO.\t8, 19 SET BATTEN_부분신설","18,000L_EXT 1,000 / 7.5kW x 4P","SET",2,null,0,null,0,null,0]
[null,"NO.1~4 SUSPENSION LIGHT BATTEN","18,000L / 3.75kW x 4P","SET",4,null,0,null,0,null,0]
[null,"NO.1~3 UPPER SOUND REFLECTION BOARD BATTEN","14,200L, 12,000L                         / 3.75kW x 4P","SET",3,null,0,null,0,null,0]
[null,"UPPER HORIZONT LIGHT BATTEN","18,000L / 3.75kW x 4P","SET",1,null,0,null,0,null,0]
[null,"NO.1~2 HORIZONT CURTAIN BATTEN","18,000L / 3.75kW x 4P","SET",2,null,0,null,0,null,0]
[null,"GRID IRON 보강",null,"식",1,null,0,null,0,null,0]
[null,"MAIN POWER PANEL",null,"식",1,null,0,null,0,null,0]
[null,"MCC PANEL"," ","SET",1,null,0,null,0,null,0]
[null,"MOTION CONTROL PANEL"," ","SET",1,null,0,null,0,null,0]
[null,"MAIN CONTROL CONSOLE"," ","SET",1,null,0,null,0,null,0]
[null,"PIPING & WIRING",null,"식",1,null,0,null,0,null,0]
[null,"기존무대장치 철거 및 고철처리비 정산",null,"식",1,null,0,null,0,null,0]
[null,"무대바닥 보양작업",null,"식",1,null,0,{"$nulls":3},0]
[]
[null,"소         계"]
[null,"부가가치세"]
[null,"합        계",{"$nulls":4},0,null,0,null,0]